|  |  |
| --- | --- |
|  | **Injury & Illness Prevention Program**Job Safety Analysis Form |
| 1000 E Victoria St.• Carson, CA 90747Phone: 310-243-3000 • Office: 310-243-3171 www.csudh.edu/ehs |

|  |  |  |
| --- | --- | --- |
| **Picture of task/equipment:** | **Task:** | Stihl Gas Powered Hedge Trimmer |
| Stihl HL 91 K (0°) Professional Hedge Trimmer Double-Sided 24.1cc | **Name of Shop or Dept:** | CSUDH Campus - Grounds |
| **Job Title(s):** |  |
| **Analyzed by:** | Orson Faynor |
| **Date:** | 11/9/2021 |
| **Required PPE:** |
|

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Work Boots** | **Gloves** | **Hearing Protection** | **Safety Glasses** | **Safety Vest** | **Mask/Face Protection** |
| Wolverine | 6 in Work Boot, 12, M, Men's, Brown, Steel Toe Type, 1 PR [PK/1] Model: W08289 |Grainger | Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902 | http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600 | Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110 |  | Nuisance Removal Dust Mask, PK 50 |
| [x]  | [x]  | [ ]  | [x]  | [ ]  | [ ]  |

 |
| **Required/Recommended Trainings:** |
|  **IIPP Equipment Specific** |
| **TASK** | **HAZARDS** | **CONTROLS** |
|  UseNew Stihl HS 82 R 30 in. Power Equipment in Greenville, NC | Stock Number: | AmputationsLacerationsFalls | Do not operate machine when fatigued. If you are tired, take a break. Tiredness may result in loss of control.To reduce the risk of injury from blade contact, never carry or transport power tool with the blades moving.Before starting machine be sure the cutting tool is clear of you and all other obstructions and objects to prevent blade contact.Always hold the unit firmly with both hands on the handles when you are working. Wrap your fingers and thumbs around the handles.Always operate the machine so that the cutting blades are away from your body.Do not overreach. Keep proper footing and balance at all times. Special care must be taken in slippery conditions and in difficult, overgrown terrain. Be extremely cautious when working on slopes and uneven ground.To reduce the risk of injury from loss of control, never work on a ladder, in a tree or any other insecure support. Never hold the machine above shoulder height.Always stop the engine and make sure the cutting blades are stopped before doing any maintenance or repair work or cleaning the tool. |