|  |  |
| --- | --- |
|  | **Injury & Illness Prevention Program**Job Safety Analysis Form |
| 1000 E Victoria St.• Carson, CA 90747 Phone: 310-243-3000 • Office: 310-243-3171[www.csudh.edu/ehs](http://www.csudh.edu/ehs) |
|  |
| **Picture of task/equipment:** | **Task:** | Dumping waste with Vestil JMD-1000 |
|  | **Name of Shop****or Dept:** | CSUDH Campus - Sustainability |
| **Job Title(s):** | Sustainability, Mover |
| **Analyzed by:** | M. Williams |
| **Date:** | 5/11/2022 |
| **Required PPE:** |
| **Work Boots Gloves Hearing Protection Safety Glasses Safety Vest Mask/Face Protection**Wolverine | 6 in Work Boot, 12, M, Men's, Brown, Steel Toe Type, 1 PR [PK/1] Model: W08289 |Grainger Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902  Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110  ☒ ☐ ☐ ☒ ☐ ☐ |
| **Required/Recommended Trainings:** |
| **IIPP Equipment Specific** |
| **TASK** | **HAZARDS** | **CONTROLS** |
| Dumping waste in the Vestil JMD-1000 tote dumper | Struck By’s Pinch Lacerations | D Inspect the tote for damage before each lift. Do not attempt to pick up the tote unless it is in good condition.D Always have the floor lock engaged solidly with the floor surface when the dumper is in operation.D Lock wheels before operationD Verify that the tote is engaged and held securely by the dumper before proceeding to raise the tote.D Always watch the dumper and the tote carefully when the dumper is in operation.D Stand away from the side of the dumper when it is in operation. Stay clear of any potential pinch and shear points.D Be alert to the possibility of splashing or flying material when dumping loads.D Do not use the dumper if any damage or unusual noise is observed.D When moving the dumper for charging, raise handlebar and push dumper to charging stationD Ensure wheels are locked when charging |